Thanks for purchasing PLANET FGSW-2620PVM Layer 2 Management Ethernet Switch.
This document provides the firmware release note and history of the product

Version 1.10 Released at 2009/07/08

Firmware version: 1.10
Hardware version: 1.0
Release at 2009/07/08

This firmware provides the following modification:

A. Bug Fixed -
- N/A

B. Function Added -
- N/A


[Upgrade Requirements]:

1. The latest firmware version of FGSW-2620PVM
2. The FGSW-2620PVM switch
3. Workstation with Microsoft IE 6.0 or above.
4. TFTP server. (If you want to upgrade firmware via TFTP)


[Upgrade procedure]:

1. Connect the RJ-45 UTP cable to the target switch.

2. Login is required to access the WEB interface after the switch boot completes successfully. The factory default user name and password is "admin".

3. After Web main screen appeared, click the "System --> Firmware Upgrade" at the left Menu.  

4. The screen provided HTTP Firmware Upgrade and TFTP Firmware Upgrade.

   A. HTTP Firmware Upgrade
     (1) Enter the "Browse.." button to locate firmware path.
     (2) Click "Submit" button to start the firmware upgrade procedure.Please don't power off the switch while procedure be started.
     (3) Please wait until the system reboot complete.
     (4) Reset to factory default again.

   B.TFTP Firmware Upgared

     (1) Enter the "TFTP Server IP Address" and filename with the correct firmware file.
     (2) Click "Apply" button to start the firmware upgrade procedure. Please don't power off the switch while procedure be started.
     (3) Please wait until the successful message shows in the Update Status web page.
     (4) Please wait until the system reboot complete.
     (5) Reset to factory default again.

5. Relogin the switch via WEB browser. Please click the "System -->System Information --> Firmware Version" to double check if the firmware be upgraded successfully.
 

*************************
Firmware Release History:  
*************************

Firmware version: 1.20
Hardware version: 1.0
Release at 2010/01/28 

This firmware provides the following modification:

A. Bug Fixed - 

1. Fix Switch panel location in Web UI. 
2. Fix Power Allocation could not display correct power consumption of the support POE power class PD device.
3. Fix system could not delete 11th VLAN entry at VLAN Information. 

B. Function Added - N/A


Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw


